--------------------------------------------------------------------------------
Library :MurataDynamicModel_C
Conponent name : GGD18_D
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of GGD18_D

PartNumber | tmpr | Type | Size | TempCharacteristics | RatedVoltage | Value | Tolerance | Dimensions | FreqRange
GGD188R71H102KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 1000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GGD188R72A102KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 1000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GGD188R71H222KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 2200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GGD188R72A222KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 2200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GGD188R71H472KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 4700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GGD188R72A472KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 4700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GGD188R71H103KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 10000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GGD188R72A103KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 10000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GGD188R71H223KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 50[V] | 22000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GGD188R72A223KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 100[V] | 22000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GGD188R71E473KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 1608[mm]/0603[inch] | X7R(-55to125[deg]) | 25[V] | 47000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]