--------------------------------------------------------------------------------
Library :MurataDynamicModel_C
Conponent name : GGD21_D
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of GGD21_D

PartNumber | tmpr | Type | Size | TempCharacteristics | RatedVoltage | Value | Tolerance | Dimensions | FreqRange
GGD21BR71H473KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 47000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GGD21BR72A473KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 47000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GGD21BR71H104KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 100000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GGD21BR72A104KA02 | 25 | Water repellent type and specially designed product to reduce shorts | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 100000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]