--------------------------------------------------------------------------------
Library :MurataDynamicModel_C
Conponent name : GCH32_D
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of GCH32_D

PartNumber | tmpr | Type | Size | TempCharacteristics | RatedVoltage | Value | Tolerance | Dimensions | FreqRange
GCH32ER71H475KE01 | 25 | For implantable Medical Devices (Non-critical circuits) | 3225[mm]/1210[inch] | X7R(-55to125[deg]) | 50[V] | 4700000[pF] | +/-10[%] | 3.2x2.5[mm] | 100[Hz]-6[GHz]
GCH32ER71A226KE01 | 25 | For implantable Medical Devices (Non-critical circuits) | 3225[mm]/1210[inch] | X7R(-55to125[deg]) | 10[V] | 22000000[pF] | +/-10[%] | 3.2x2.5[mm] | 100[Hz]-6[GHz]
GCH32ER70J476KE01 | 25 | For implantable Medical Devices (Non-critical circuits) | 3225[mm]/1210[inch] | X7R(-55to125[deg]) | 6.3[V] | 47000000[pF] | +/-10[%] | 3.2x2.5[mm] | 100[Hz]-6[GHz]