--------------------------------------------------------------------------------
Library :MurataDynamicModel_C
Conponent name : GCH31_D
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of GCH31_D

PartNumber | tmpr | Type | Size | TempCharacteristics | RatedVoltage | Value | Tolerance | Dimensions | FreqRange
GCH31MR72A224KE01 | 25 | For implantable Medical Devices (Non-critical circuits) | 3216[mm]/1206[inch] | X7R(-55to125[deg]) | 100[V] | 220000[pF] | +/-10[%] | 3.2x1.6[mm] | 100[Hz]-6[GHz]
GCH31CR71H225KE01 | 25 | For implantable Medical Devices (Non-critical circuits) | 3216[mm]/1206[inch] | X7R(-55to125[deg]) | 50[V] | 2200000[pF] | +/-10[%] | 3.2x1.6[mm] | 100[Hz]-6[GHz]
GCH31CR71C106KE01 | 25 | For implantable Medical Devices (Non-critical circuits) | 3216[mm]/1206[inch] | X7R(-55to125[deg]) | 16[V] | 10000000[pF] | +/-10[%] | 3.2x1.6[mm] | 100[Hz]-6[GHz]
GCH31CR60J226KE01 | 25 | For implantable Medical Devices (Non-critical circuits) | 3216[mm]/1206[inch] | X5R(-55to85[deg]) | 6.3[V] | 22000000[pF] | +/-10[%] | 3.2x1.6[mm] | 100[Hz]-6[GHz]
GCH31CR61C226ME11 | 25 | For implantable Medical Devices (Non-critical circuits) | 3216[mm]/1206[inch] | X5R(-55to85[deg]) | 16[V] | 22000000[pF] | +/-20[%] | 3.2x1.6[mm] | 100[Hz]-6[GHz]