--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM21AG
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM21AG

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM21AG102BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM21AG102SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM21AG102SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM21AG121BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM21AG121SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM21AG121SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM21AG151BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM21AG151SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM21AG151SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM21AG221BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 900[mA] | 1[MHz]-3[GHz]
BLM21AG221SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 900[mA] | 1[MHz]-3[GHz]
BLM21AG221SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 900[mA] | 1[MHz]-3[GHz]
BLM21AG331BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 800[mA] | 1[MHz]-3[GHz]
BLM21AG331SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 800[mA] | 1[MHz]-3[GHz]
BLM21AG331SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 800[mA] | 1[MHz]-3[GHz]
BLM21AG471BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM21AG471SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM21AG471SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM21AG601BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM21AG601SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM21AG601SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 700[mA] | 1[MHz]-3[GHz]