--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM41PG
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM41PG

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM41PG102SH1 | Ferrite Bead Single Type | 4516[mm]/1806[inch] | 4.5x1.6[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM41PG102SZ1 | Ferrite Bead Single Type | 4516[mm]/1806[inch] | 4.5x1.6[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM41PG181SH1 | Ferrite Bead Single Type | 4516[mm]/1806[inch] | 4.5x1.6[mm] | 3500[mA] | 1[MHz]-3[GHz]
BLM41PG181SZ1 | Ferrite Bead Single Type | 4516[mm]/1806[inch] | 4.5x1.6[mm] | 3500[mA] | 1[MHz]-3[GHz]
BLM41PG471SH1 | Ferrite Bead Single Type | 4516[mm]/1806[inch] | 4.5x1.6[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM41PG471SZ1 | Ferrite Bead Single Type | 4516[mm]/1806[inch] | 4.5x1.6[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM41PG600SH1 | Ferrite Bead Single Type | 4516[mm]/1806[inch] | 4.5x1.6[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM41PG600SZ1 | Ferrite Bead Single Type | 4516[mm]/1806[inch] | 4.5x1.6[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM41PG750SH1 | Ferrite Bead Single Type | 4516[mm]/1806[inch] | 4.5x1.6[mm] | 3500[mA] | 1[MHz]-3[GHz]
BLM41PG750SZ1 | Ferrite Bead Single Type | 4516[mm]/1806[inch] | 4.5x1.6[mm] | 3500[mA] | 1[MHz]-3[GHz]