--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM03HG
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM03HG

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM03HG102SH1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 125[mA] | 1[MHz]-3[GHz]
BLM03HG102SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 125[mA] | 1[MHz]-3[GHz]
BLM03HG122SH1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 100[mA] | 1[MHz]-3[GHz]
BLM03HG122SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 100[mA] | 1[MHz]-3[GHz]
BLM03HG601SH1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM03HG601SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 150[mA] | 1[MHz]-3[GHz]