--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM15PE
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM15PE

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM15PE121SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM15PE181SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1200[mA] | 1[MHz]-3[GHz]
BLM15PE221SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1100[mA] | 1[MHz]-3[GHz]
BLM15PE300SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 2300[mA] | 1[MHz]-3[GHz]
BLM15PE331SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM15PE471SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 750[mA] | 1[MHz]-3[GHz]
BLM15PE600SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1800[mA] | 1[MHz]-3[GHz]
BLM15PE601SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM15PE800SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1700[mA] | 1[MHz]-3[GHz]