--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM21PG
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM21PG

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM21PG121BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1550[mA] | 1[MHz]-3[GHz]
BLM21PG121SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 3000[mA] | 1[MHz]-3[GHz]
BLM21PG121SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 3000[mA] | 1[MHz]-3[GHz]
BLM21PG220BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 3300[mA] | 1[MHz]-3[GHz]
BLM21PG220SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM21PG220SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM21PG221BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1250[mA] | 1[MHz]-3[GHz]
BLM21PG221SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM21PG221SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM21PG300BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 2300[mA] | 1[MHz]-3[GHz]
BLM21PG300SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 4000[mA] | 1[MHz]-3[GHz]
BLM21PG300SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 4000[mA] | 1[MHz]-3[GHz]
BLM21PG331BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM21PG331SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM21PG331SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM21PG600BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1900[mA] | 1[MHz]-3[GHz]
BLM21PG600SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 3500[mA] | 1[MHz]-3[GHz]
BLM21PG600SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 3500[mA] | 1[MHz]-3[GHz]
BLM21PG102BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1150[mA] | 1[MHz]-3[GHz]
BLM21PG601BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1400[mA] | 1[MHz]-3[GHz]
BLM21PG102SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1150[mA] | 1[MHz]-3[GHz]
BLM21PG601SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1400[mA] | 1[MHz]-3[GHz]