--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM21SP
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM21SP

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM21SP102BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1600[mA] | 1[MHz]-3[GHz]
BLM21SP102SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1600[mA] | 1[MHz]-3[GHz]
BLM21SP102SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1600[mA] | 1[MHz]-3[GHz]
BLM21SP111BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 5000[mA] | 1[MHz]-3[GHz]
BLM21SP111SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 5000[mA] | 1[MHz]-3[GHz]
BLM21SP111SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 5000[mA] | 1[MHz]-3[GHz]
BLM21SP181BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 4000[mA] | 1[MHz]-3[GHz]
BLM21SP181SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 4000[mA] | 1[MHz]-3[GHz]
BLM21SP181SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 4000[mA] | 1[MHz]-3[GHz]
BLM21SP331BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 2800[mA] | 1[MHz]-3[GHz]
BLM21SP331SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 2800[mA] | 1[MHz]-3[GHz]
BLM21SP331SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 2800[mA] | 1[MHz]-3[GHz]
BLM21SP471BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 2500[mA] | 1[MHz]-3[GHz]
BLM21SP471SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 2500[mA] | 1[MHz]-3[GHz]
BLM21SP471SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 2500[mA] | 1[MHz]-3[GHz]
BLM21SP601BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 2300[mA] | 1[MHz]-3[GHz]
BLM21SP601SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 2300[mA] | 1[MHz]-3[GHz]
BLM21SP601SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 2300[mA] | 1[MHz]-3[GHz]
BLM21SP700BH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM21SP700SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM21SP700SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 6000[mA] | 1[MHz]-3[GHz]