--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM18HG
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM18HG

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM18HG102SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 100[mA] | 1[MHz]-3[GHz]
BLM18HG102SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 100[mA] | 1[MHz]-3[GHz]
BLM18HG471SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM18HG471SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM18HG601SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM18HG601SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]