--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM15PX
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM15PX

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM15PX121SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM15PX181SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM15PX221SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1400[mA] | 1[MHz]-3[GHz]
BLM15PX330SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 3000[mA] | 1[MHz]-3[GHz]
BLM15PX331SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1200[mA] | 1[MHz]-3[GHz]
BLM15PX471SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM15PX600SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 2500[mA] | 1[MHz]-3[GHz]
BLM15PX601SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 900[mA] | 1[MHz]-3[GHz]
BLM15PX800SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 2300[mA] | 1[MHz]-3[GHz]
BLM15PX121SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM15PX181SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM15PX221SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1400[mA] | 1[MHz]-3[GHz]
BLM15PX330SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 3000[mA] | 1[MHz]-3[GHz]
BLM15PX331SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1200[mA] | 1[MHz]-3[GHz]
BLM15PX471SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM15PX600SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 2500[mA] | 1[MHz]-3[GHz]
BLM15PX601SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 900[mA] | 1[MHz]-3[GHz]
BLM15PX800SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 2300[mA] | 1[MHz]-3[GHz]
BLM15PX121BH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM15PX181BH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM15PX221BH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1400[mA] | 1[MHz]-3[GHz]
BLM15PX330BH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 3000[mA] | 1[MHz]-3[GHz]
BLM15PX331BH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1200[mA] | 1[MHz]-3[GHz]
BLM15PX471BH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM15PX600BH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 2500[mA] | 1[MHz]-3[GHz]
BLM15PX601BH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 900[mA] | 1[MHz]-3[GHz]
BLM15PX800BH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 2300[mA] | 1[MHz]-3[GHz]