--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM02PX
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM02PX

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM02PX100SN1 | Ferrite Bead Single Type | 0402[mm]/01005[inch] | 0.4x0.2[mm] | 1100[mA] | 1[MHz]-3[GHz]
BLM02PX220SN1 | Ferrite Bead Single Type | 0402[mm]/01005[inch] | 0.4x0.2[mm] | 750[mA] | 1[MHz]-3[GHz]
BLM02PX330SN1 | Ferrite Bead Single Type | 0402[mm]/01005[inch] | 0.4x0.2[mm] | 550[mA] | 1[MHz]-3[GHz]
BLM02PX600SN1 | Ferrite Bead Single Type | 0402[mm]/01005[inch] | 0.4x0.2[mm] | 500[mA] | 1[MHz]-3[GHz]