--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM21BB
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM21BB

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM21BB050SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM21BB050SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM21BB121SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM21BB121SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM21BB151SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM21BB151SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM21BB201SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM21BB201SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM21BB221SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM21BB221SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM21BB331SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 400[mA] | 1[MHz]-3[GHz]
BLM21BB331SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 400[mA] | 1[MHz]-3[GHz]
BLM21BB471SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 400[mA] | 1[MHz]-3[GHz]
BLM21BB471SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 400[mA] | 1[MHz]-3[GHz]
BLM21BB600SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 800[mA] | 1[MHz]-3[GHz]
BLM21BB600SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 800[mA] | 1[MHz]-3[GHz]
BLM21BB750SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM21BB750SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 700[mA] | 1[MHz]-3[GHz]