--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM18KN
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM18KN

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM18KN101EH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1900[mA] | 1[MHz]-3[GHz]
BLM18KN102EH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 740[mA] | 1[MHz]-3[GHz]
BLM18KN121EH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1900[mA] | 1[MHz]-3[GHz]
BLM18KN221EH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1400[mA] | 1[MHz]-3[GHz]
BLM18KN260EH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 4000[mA] | 1[MHz]-3[GHz]
BLM18KN300EH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2600[mA] | 1[MHz]-3[GHz]
BLM18KN331EH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1100[mA] | 1[MHz]-3[GHz]
BLM18KN471EH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 920[mA] | 1[MHz]-3[GHz]
BLM18KN601EH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 860[mA] | 1[MHz]-3[GHz]
BLM18KN700EH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2200[mA] | 1[MHz]-3[GHz]