--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM15AG
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM15AG

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM15AG100SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM15AG100SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM15AG102SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM15AG102SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM15AG121SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM15AG121SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 550[mA] | 1[MHz]-3[GHz]
BLM15AG221SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM15AG221SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 450[mA] | 1[MHz]-3[GHz]
BLM15AG601SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM15AG601SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM15AG700SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM15AG700SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 600[mA] | 1[MHz]-3[GHz]