--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM03AG
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM03AG

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM03AG100SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM03AG102SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 100[mA] | 1[MHz]-3[GHz]
BLM03AG121SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM03AG241SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM03AG601SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 100[mA] | 1[MHz]-3[GHz]
BLM03AG700SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM03AG800SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 200[mA] | 1[MHz]-3[GHz]