--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM31KN
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM31KN

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM31KN102BH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 1400[mA] | 1[MHz]-3[GHz]
BLM31KN102SH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM31KN102SZ1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM31KN121BH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 4000[mA] | 1[MHz]-3[GHz]
BLM31KN121SH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM31KN121SZ1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM31KN271BH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 3000[mA] | 1[MHz]-3[GHz]
BLM31KN271SH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 4500[mA] | 1[MHz]-3[GHz]
BLM31KN271SZ1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 4500[mA] | 1[MHz]-3[GHz]
BLM31KN471BH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 2700[mA] | 1[MHz]-3[GHz]
BLM31KN471SH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 4000[mA] | 1[MHz]-3[GHz]
BLM31KN471SZ1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 4000[mA] | 1[MHz]-3[GHz]
BLM31KN601BH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM31KN601SH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 2900[mA] | 1[MHz]-3[GHz]
BLM31KN601SZ1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 2900[mA] | 1[MHz]-3[GHz]
BLM31KN801BH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 1700[mA] | 1[MHz]-3[GHz]
BLM31KN801SH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 2500[mA] | 1[MHz]-3[GHz]
BLM31KN801SZ1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 2500[mA] | 1[MHz]-3[GHz]