--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM31PG
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM31PG

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM31PG121SH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 3500[mA] | 1[MHz]-3[GHz]
BLM31PG121SZ1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 3500[mA] | 1[MHz]-3[GHz]
BLM31PG330SH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM31PG330SZ1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM31PG391SH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM31PG391SZ1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM31PG500SH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 3500[mA] | 1[MHz]-3[GHz]
BLM31PG500SZ1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 3500[mA] | 1[MHz]-3[GHz]
BLM31PG601SH1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM31PG601SZ1 | Ferrite Bead Single Type | 3216[mm]/1206[inch] | 3.2x1.6[mm] | 1500[mA] | 1[MHz]-3[GHz]