--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM18SP
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM18SP

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM18SP101SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 3700[mA] | 1[MHz]-3[GHz]
BLM18SP101SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 3700[mA] | 1[MHz]-3[GHz]
BLM18SP102SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1200[mA] | 1[MHz]-3[GHz]
BLM18SP102SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1200[mA] | 1[MHz]-3[GHz]
BLM18SP221SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2800[mA] | 1[MHz]-3[GHz]
BLM18SP221SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2800[mA] | 1[MHz]-3[GHz]
BLM18SP300SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM18SP300SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM18SP601SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM18SP601SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1500[mA] | 1[MHz]-3[GHz]