--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM18AG
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM18AG

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM18AG102BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 450[mA] | 1[MHz]-3[GHz]
BLM18AG102SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 450[mA] | 1[MHz]-3[GHz]
BLM18AG102SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 450[mA] | 1[MHz]-3[GHz]
BLM18AG102WH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM18AG121BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 800[mA] | 1[MHz]-3[GHz]
BLM18AG121SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 800[mA] | 1[MHz]-3[GHz]
BLM18AG121SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 800[mA] | 1[MHz]-3[GHz]
BLM18AG151BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM18AG151SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM18AG151SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM18AG221BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM18AG221SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM18AG221SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM18AG331BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM18AG331SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM18AG331SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM18AG471BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 550[mA] | 1[MHz]-3[GHz]
BLM18AG471SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 550[mA] | 1[MHz]-3[GHz]
BLM18AG471SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 550[mA] | 1[MHz]-3[GHz]
BLM18AG471WH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM18AG601BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18AG601SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18AG601SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]