--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM02AX
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM02AX

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM02AX100SN1 | Ferrite Bead Single Type | 0402[mm]/01005[inch] | 0.4x0.2[mm] | 750[mA] | 1[MHz]-3[GHz]
BLM02AX121SN1 | Ferrite Bead Single Type | 0402[mm]/01005[inch] | 0.4x0.2[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM02AX241SN1 | Ferrite Bead Single Type | 0402[mm]/01005[inch] | 0.4x0.2[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM02AX700SN1 | Ferrite Bead Single Type | 0402[mm]/01005[inch] | 0.4x0.2[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM02AX331SN1 | Ferrite Bead Single Type | 0402[mm]/01005[inch] | 0.4x0.2[mm] | 150[mA] | 1[MHz]-3[GHz]