--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM15AX
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM15AX

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM15AX100SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1740[mA] | 1[MHz]-3[GHz]
BLM15AX102SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 350[mA] | 1[MHz]-3[GHz]
BLM15AX121SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM15AX221SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM15AX300SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 1100[mA] | 1[MHz]-3[GHz]
BLM15AX601SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM15AX700SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 780[mA] | 1[MHz]-3[GHz]