--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM15HG
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM15HG

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM15HG102BH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM15HG102SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM15HG102SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM15HG601BH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM15HG601SH1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM15HG601SZ1 | Ferrite Bead Single Type | 1005[mm]/0402[inch] | 1.0x0.5[mm] | 300[mA] | 1[MHz]-3[GHz]