--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM18KG
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM18KG

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM18KG101JH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1900[mA] | 1[MHz]-3[GHz]
BLM18KG101TH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 3000[mA] | 1[MHz]-3[GHz]
BLM18KG101TZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 3000[mA] | 1[MHz]-3[GHz]
BLM18KG101WH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM18KG102BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 800[mA] | 1[MHz]-3[GHz]
BLM18KG102SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM18KG102SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM18KG102WH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 800[mA] | 1[MHz]-3[GHz]
BLM18KG121JH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1900[mA] | 1[MHz]-3[GHz]
BLM18KG121TH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 3000[mA] | 1[MHz]-3[GHz]
BLM18KG121TZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 3000[mA] | 1[MHz]-3[GHz]
BLM18KG121WH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM18KG221BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM18KG221SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2200[mA] | 1[MHz]-3[GHz]
BLM18KG221SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2200[mA] | 1[MHz]-3[GHz]
BLM18KG221WH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1400[mA] | 1[MHz]-3[GHz]
BLM18KG260JH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 4000[mA] | 1[MHz]-3[GHz]
BLM18KG260TH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM18KG260TZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 6000[mA] | 1[MHz]-3[GHz]
BLM18KG260WH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM18KG300JH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 3300[mA] | 1[MHz]-3[GHz]
BLM18KG300TH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 5000[mA] | 1[MHz]-3[GHz]
BLM18KG300TZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 5000[mA] | 1[MHz]-3[GHz]
BLM18KG300WH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1850[mA] | 1[MHz]-3[GHz]
BLM18KG331BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1200[mA] | 1[MHz]-3[GHz]
BLM18KG331SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1700[mA] | 1[MHz]-3[GHz]
BLM18KG331SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1700[mA] | 1[MHz]-3[GHz]
BLM18KG331WH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1250[mA] | 1[MHz]-3[GHz]
BLM18KG471BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM18KG471SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM18KG471SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1500[mA] | 1[MHz]-3[GHz]
BLM18KG471WH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1100[mA] | 1[MHz]-3[GHz]
BLM18KG601BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM18KG601SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1300[mA] | 1[MHz]-3[GHz]
BLM18KG601SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1300[mA] | 1[MHz]-3[GHz]
BLM18KG601WH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM18KG700JH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2200[mA] | 1[MHz]-3[GHz]
BLM18KG700TH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 3500[mA] | 1[MHz]-3[GHz]
BLM18KG700TZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 3500[mA] | 1[MHz]-3[GHz]
BLM18KG700WH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1650[mA] | 1[MHz]-3[GHz]