--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM03AX
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM03AX

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM03AX100SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM03AX102SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM03AX121SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 450[mA] | 1[MHz]-3[GHz]
BLM03AX241SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 350[mA] | 1[MHz]-3[GHz]
BLM03AX601SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM03AX800SZ1 | Ferrite Bead Single Type | 0603[mm]/0201[inch] | 0.6x0.3[mm] | 500[mA] | 1[MHz]-3[GHz]