--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM18BD
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM18BD

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM18BD102BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM18BD102SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM18BD102SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM18BD121BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM18BD121SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM18BD121SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM18BD151BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM18BD151SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM18BD151SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM18BD152BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM18BD152SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM18BD152SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM18BD182BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM18BD182SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM18BD182SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM18BD221BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM18BD221SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM18BD221SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM18BD222BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM18BD222SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM18BD222SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM18BD252BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM18BD252SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM18BD252SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 150[mA] | 1[MHz]-3[GHz]
BLM18BD331BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM18BD331SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM18BD331SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM18BD421BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM18BD421SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM18BD421SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM18BD470BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18BD470SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18BD470SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18BD471BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM18BD471SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM18BD471SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM18BD601BH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM18BD601SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM18BD601SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]