--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM18BA
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM18BA

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM18BA050SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18BA050SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18BA100SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18BA100SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18BA121SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM18BA121SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM18BA220SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18BA220SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18BA470SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM18BA470SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM18BA750SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM18BA750SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 300[mA] | 1[MHz]-3[GHz]