--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM18EG
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM18EG

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM18EG101TH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM18EG101TZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM18EG121SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM18EG121SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM18EG181SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM18EG221SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 2000[mA] | 1[MHz]-3[GHz]
BLM18EG221TH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM18EG221TZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 1000[mA] | 1[MHz]-3[GHz]
BLM18EG331TH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18EG331TZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18EG391TH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18EG391TZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18EG471SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18EG471SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18EG601SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18EG601SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]