--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM18BB
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM18BB

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM18BB050SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 800[mA] | 1[MHz]-3[GHz]
BLM18BB050SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 800[mA] | 1[MHz]-3[GHz]
BLM18BB100SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM18BB100SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM18BB121SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 550[mA] | 1[MHz]-3[GHz]
BLM18BB121SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 550[mA] | 1[MHz]-3[GHz]
BLM18BB141SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18BB141SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 500[mA] | 1[MHz]-3[GHz]
BLM18BB151SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 450[mA] | 1[MHz]-3[GHz]
BLM18BB151SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 450[mA] | 1[MHz]-3[GHz]
BLM18BB220SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM18BB220SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 700[mA] | 1[MHz]-3[GHz]
BLM18BB221SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 450[mA] | 1[MHz]-3[GHz]
BLM18BB221SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 450[mA] | 1[MHz]-3[GHz]
BLM18BB331SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 400[mA] | 1[MHz]-3[GHz]
BLM18BB331SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 400[mA] | 1[MHz]-3[GHz]
BLM18BB470SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM18BB470SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM18BB471SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM18BB471SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM18BB600SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM18BB600SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM18BB750SH1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 600[mA] | 1[MHz]-3[GHz]
BLM18BB750SZ1 | Ferrite Bead Single Type | 1608[mm]/0603[inch] | 1.6x0.8[mm] | 600[mA] | 1[MHz]-3[GHz]