--------------------------------------------------------------------------------
Library :muRataLibWeb_L
Conponent name : BLM21BD
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of BLM21BD

PartNumber | Type | Size | Dimensions | RatedCurrent | FreqRange
BLM21BD102SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM21BD102SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM21BD121SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 350[mA] | 1[MHz]-3[GHz]
BLM21BD121SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 350[mA] | 1[MHz]-3[GHz]
BLM21BD151SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 350[mA] | 1[MHz]-3[GHz]
BLM21BD151SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 350[mA] | 1[MHz]-3[GHz]
BLM21BD152SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM21BD152SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM21BD182SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM21BD182SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM21BD221SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 350[mA] | 1[MHz]-3[GHz]
BLM21BD221SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 350[mA] | 1[MHz]-3[GHz]
BLM21BD222SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM21BD222SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM21BD222TH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM21BD222TZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM21BD272SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM21BD272SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 200[mA] | 1[MHz]-3[GHz]
BLM21BD331SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM21BD331SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM21BD421SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM21BD421SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM21BD471SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM21BD471SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM21BD601SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM21BD601SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 300[mA] | 1[MHz]-3[GHz]
BLM21BD751SH1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 250[mA] | 1[MHz]-3[GHz]
BLM21BD751SZ1 | Ferrite Bead Single Type | 2012[mm]/0805[inch] | 2.0x1.2[mm] | 250[mA] | 1[MHz]-3[GHz]