create_constant_form("NULL","NULL",16,"NULL","NULL");
create_constant_form("LQW18FTR55K0H","1:LQW18FTR55K0H, Wound, 550[nH], +/-10[%], 800[mA], 0.1[MHz]-20[GHz]:1",68,"1","LQW18FTR55K0H");
create_constant_form("LQW18FT1R2K0H","2:LQW18FT1R2K0H, Wound, 1200[nH], +/-10[%], 560[mA], 0.1[MHz]-20[GHz]:2",68,"2","LQW18FT1R2K0H");
create_constant_form("LQW18FT1R5K0H","3:LQW18FT1R5K0H, Wound, 1500[nH], +/-10[%], 530[mA], 0.1[MHz]-20[GHz]:3",68,"3","LQW18FT1R5K0H");
create_constant_form("LQW18FT2R2K0H","4:LQW18FT2R2K0H, Wound, 2200[nH], +/-10[%], 390[mA], 0.1[MHz]-20[GHz]:4",68,"4","LQW18FT2R2K0H");

create_form_set("LQW18FT_0H_list" 
,"LQW18FTR55K0H"
,"LQW18FT1R2K0H"
,"LQW18FT1R5K0H"
,"LQW18FT2R2K0H"
);

create_compound_form("LQW18FT_0H_compound","Discrete Optimize setting","DistLibForm",68,"%p opt{ discrete %1p to %2p by 1 }","%s, %1s to %2s",
create_parm("NOM","Nominal",32,"LQW18FT_0H_list",-1,prm("LQW18FTR55K0H")),
create_parm("MIN","Minimum",32,"LQW18FT_0H_list",-1,prm("LQW18FTR55K0H")),
create_parm("MAX","Maximum",32,"LQW18FT_0H_list",-1,prm("LQW18FT2R2K0H")));

create_form_set("LQW18FT_0H_list_opt","NULL" 
,"LQW18FTR55K0H"
,"LQW18FT1R2K0H"
,"LQW18FT1R5K0H"
,"LQW18FT2R2K0H"
,"LQW18FT_0H_compound"
);



