--------------------------------------------------------------------------------
Library :muRataLibWeb_C
Conponent name : GCE21
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of GCE21

PartNumber | Type | Size | TempCharacteristics | RatedVoltage | Value | Tolerance | Dimensions | FreqRange
GCE219R72A221KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 220[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE219R72A221MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 220[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE219R72A471KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 470[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE219R72A681KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 680[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE216R72A102KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 1000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE216R71H152KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 1500[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE216R72A152KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 1500[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE216R72A222KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 2200[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE216R71H332KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 3300[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE216R72A332KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 3300[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE216R71H392KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 3900[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE216R72A392KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 3900[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE216R71H472KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 4700[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE216R72A472KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 4700[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE219R72A682KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 6800[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A103KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 10000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H153KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 15000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A153KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 15000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H183KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 18000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H223KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 22000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A223KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 22000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H273KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 27000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H273MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 27000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A273KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 27000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A273MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 27000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H333KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 33000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H333MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 33000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A333KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 33000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A333MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 33000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H393KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 39000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H393MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 39000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A393KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 39000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A393MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 39000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H473KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 47000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H473MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 47000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A473KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 47000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A473MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 47000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H563KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 56000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H563MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 56000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A563KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 56000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A563MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 56000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H683KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 68000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H683MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 68000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A683KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 68000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A683MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 68000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H823KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 82000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H823MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 82000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A823KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 82000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A823MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 82000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H104KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 100000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR71H104MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 50[V] | 100000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A104KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 100000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCE21BR72A104MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm] | X7R(-55to125[deg]) | 100[V] | 100000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]