--------------------------------------------------------------------------------
Library :muRataLibWeb_C
Conponent name : GCJ18
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of GCJ18

PartNumber | Type | Size | TempCharacteristics | RatedVoltage | Value | Tolerance | Dimensions | FreqRange
GCJ188L81H102KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 1000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H102MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 1000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E102KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 1000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E102MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 1000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H102KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 1000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H102MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 1000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A102KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 1000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A102MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 1000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A102KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 1000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A102MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 1000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E122KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 1200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H122KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 1200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A122KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 1200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A122KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 1200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H152KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 1500[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H152MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 1500[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E152KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 1500[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E152MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 1500[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H152KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 1500[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H152MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 1500[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A152KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 1500[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A152MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 1500[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A152KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 1500[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H182KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 1800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E182KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 1800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H182KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 1800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A182KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 1800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A182KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 1800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H222KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 2200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H222MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 2200[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E222KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 2200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E222MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 2200[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H222KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 2200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H222MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 2200[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A222KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 2200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A222MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 2200[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A222KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 2200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H272KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 2700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E272KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 2700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H272KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 2700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A272KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 2700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A272KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 2700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H332KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 3300[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E332KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 3300[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H332KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 3300[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A332KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 3300[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A332KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 3300[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H392KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 3900[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E392KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 3900[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H392KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 3900[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A392KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 3900[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A392KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 3900[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H472KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 4700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H472MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 4700[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E472KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 4700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E472MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 4700[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H472KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 4700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H472MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 4700[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A472KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 4700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A472MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 4700[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91H472KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 50[V] | 4700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A472KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 4700[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A472MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 4700[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H562KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 5600[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E562KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 5600[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H562KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 5600[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A562KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 5600[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A562KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 5600[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H682KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 6800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E682KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 6800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H682KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 6800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A682KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 6800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A682KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 6800[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H822KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 8200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E822KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 8200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H822KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 8200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A822KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 8200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A822KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 8200[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H103KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 10000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H103MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 10000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C103KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 10000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C103MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 10000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E103KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 10000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E103MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 10000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H103KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 10000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H103MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 10000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A103KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 10000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A103MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 10000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91H103KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 50[V] | 10000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91H103MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 50[V] | 10000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A103KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 10000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A103MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 10000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H123KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 12000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E123KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 12000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H123KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 12000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A123KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 12000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A123KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 12000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H153KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 15000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H153MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 15000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E153KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 15000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E153MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 15000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H153KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 15000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H153MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 15000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A153KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 15000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A153MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 15000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A153KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 15000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E183KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 18000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H183KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 18000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A183KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 18000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A183KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 18000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H223KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 22000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81H223MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V] | 22000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E223KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 22000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E223MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 22000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H223KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 22000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H223MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 22000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A223KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 22000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A223MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 22000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A223KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 22000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A223MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 22000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C273KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 27000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C273MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 27000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E273KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 27000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E273MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 27000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A273KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 27000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81E333KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 25[V] | 33000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L8YA333KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 35[V] | 33000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C333KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 33000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C333MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 33000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E333KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 33000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E333MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 33000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H333KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 33000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A333KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 33000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A333MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 33000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81C393KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 16[V] | 39000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81E393KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 25[V] | 39000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L8YA393KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 35[V] | 39000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C393KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 39000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E393KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 39000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H393KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 39000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A393KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 39000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81C473KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 16[V] | 47000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81C473MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 16[V] | 47000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C473KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 47000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E473KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 47000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H473KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 47000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H473MA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 47000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A473KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 47000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A473MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 47000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81E563KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 25[V] | 56000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L8YA563KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 35[V] | 56000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C563KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 56000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E563KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 56000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H563KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 56000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A563KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 56000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81C683KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 16[V] | 68000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81C683MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 16[V] | 68000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81E683KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 25[V] | 68000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81E683MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 25[V] | 68000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L8YA683KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 35[V] | 68000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L8YA683MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 35[V] | 68000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C683KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 68000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E683KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 68000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E683MA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 68000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H683KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 68000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H683MA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 68000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R92A683KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 100[V] | 68000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81E823KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 25[V] | 82000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C823KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 82000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E823KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 82000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H823KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 82000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81C104KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 16[V] | 100000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81C104MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 16[V] | 100000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L8EL104KA07 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 100[V]_derating | 100000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C104KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 100000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E104KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 100000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E104MA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 100000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H104KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 100000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H104MA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 100000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A104KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 100000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R72A104MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 100[V] | 100000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91H104KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 50[V] | 100000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81C124KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 16[V] | 120000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71A124KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 10[V] | 120000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C124KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 120000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E124KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 120000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91H124KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 50[V] | 120000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81C154KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 16[V] | 150000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[kHz]-6[GHz]
GCJ188L81C154MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 16[V] | 150000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[kHz]-6[GHz]
GCJ188L81E154KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 25[V] | 150000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L8EH154KA07 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V]_derating | 150000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71A154KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 10[V] | 150000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[kHz]-6[GHz]
GCJ188R71A154MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 10[V] | 150000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[kHz]-6[GHz]
GCJ188R71C154KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 150000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E154KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 150000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H154KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 150000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91H154KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 50[V] | 150000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81E184KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 25[V] | 180000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C184KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 180000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E184KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 180000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91H184KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 50[V] | 180000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81C224KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 16[V] | 220000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L81E224KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 25[V] | 220000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188L8EH224KA07 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8L(-55to150[deg]) | 50[V]_derating | 220000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71A224KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 10[V] | 220000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C224KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 220000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E224KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 220000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H224KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 220000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71H224MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 50[V] | 220000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91H224KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 50[V] | 220000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91H224MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 50[V] | 220000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C274KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 270000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C334KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 330000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C334MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 330000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91E334KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 25[V] | 330000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91E334MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 25[V] | 330000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C394KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 390000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C394MA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 390000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91E394KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 25[V] | 390000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C474KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 470000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71C474MA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 16[V] | 470000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91E474KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 25[V] | 470000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R91E474MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8R(-55to150[deg]) | 25[V] | 470000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E105KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 1000000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R71E105MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 25[V] | 1000000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R70J225KE01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 6.3[V] | 2200000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188R70J225ME01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7R(-55to125[deg]) | 6.3[V] | 2200000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188C70J335KE02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7S(-55to125[deg]) | 6.3[V] | 3300000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188C70J335ME02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7S(-55to125[deg]) | 6.3[V] | 3300000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188C70J475KE02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7S(-55to125[deg]) | 6.3[V] | 4700000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188C70J475ME02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7S(-55to125[deg]) | 6.3[V] | 4700000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188M8EC475KE08 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X8M(-55to150[deg]) | 6.3[V]_derating | 4700000[pF] | +/-10[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]
GCJ188D70J106ME02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 1608[mm] | X7T(-55to125[deg]) | 6.3[V] | 10000000[pF] | +/-20[%] | 1.6x0.8[mm] | 100[Hz]-6[GHz]