--------------------------------------------------------------------------------
Library :muRataLibWeb_C
Conponent name : GCJ21
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of GCJ21

PartNumber | Type | Size | TempCharacteristics | RatedVoltage | Value | Tolerance | Dimensions | FreqRange
GCJ219R72A221KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 220[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A221MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 220[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A271KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 270[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H331KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 330[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H331MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 330[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A331KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 330[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A391KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 390[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E471KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 470[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E471MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 470[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H471KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 470[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H471MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 470[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A471KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 470[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A471MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 470[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E561KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 560[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E561MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 560[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H561KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 560[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H561MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 560[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A561KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 560[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A681KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 680[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A681MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 680[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E821KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 820[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H821KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 820[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A821KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 820[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E102KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 1000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E102MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 1000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H102KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 1000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H102MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 1000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A102KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 1000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A102MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 1000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21AR72E102KXJ1 | 200V and over/ Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 250[V] | 1000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-3[GHz]
GCJ216R72A122KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 1200[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A152KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 1500[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21AR72E152KXJ1 | 200V and over/ Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 250[V] | 1500[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-3[GHz]
GCJ216R72A182KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 1800[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E222KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 2200[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E222MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 2200[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H222KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 2200[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H222MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 2200[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A222KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 2200[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A222MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 2200[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21AR72E222KXJ1 | 200V and over/ Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 250[V] | 2200[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-3[GHz]
GCJ216R72A272KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 2700[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E332KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 3300[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E332MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 3300[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H332KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 3300[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H332MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 3300[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A332KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 3300[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A332MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 3300[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21AR72E332KXJ1 | 200V and over/ Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 250[V] | 3300[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-3[GHz]
GCJ216R72A392KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 3900[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E472KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 4700[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E472MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 4700[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H472KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 4700[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H472MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 4700[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A472KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 4700[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A472MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 4700[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21AR72E472KXJ1 | 200V and over/ Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 250[V] | 4700[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-3[GHz]
GCJ216R72A562KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 5600[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E682KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 6800[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E682MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 6800[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H682KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 6800[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H682MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 6800[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A682KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 6800[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A682MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 6800[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21AR72E682KXJ1 | 200V and over/ Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 250[V] | 6800[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-3[GHz]
GCJ216R72A822KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 8200[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E103KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 10000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71E103MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 10000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H103KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 10000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H103MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 10000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A103KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 10000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A103MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 10000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR72E103KXJ3 | 200V and over/ Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 250[V] | 10000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-3[GHz]
GCJ216R72A123KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 12000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H153KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 15000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H153MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 15000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A153KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 15000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A153MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 15000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR72E153KXJ3 | 200V and over/ Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 250[V] | 15000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-3[GHz]
GCJ216R72A183KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 18000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R71E223KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 22000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R71E223MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 22000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H223KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 22000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R71H223MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 22000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A223KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 22000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ216R72A223MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 22000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR72E223KXJ3 | 200V and over/ Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 250[V] | 22000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-3[GHz]
GCJ21BL81H273KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 50[V] | 27000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E273KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 27000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R71H273KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 27000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R71H273MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 27000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A273KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 27000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A273MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 27000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R71H333KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 33000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R71H333MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 33000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A333KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 33000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A333MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 33000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81H393KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 50[V] | 39000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R71H393KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 39000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R72A393KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 39000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81H473KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 50[V] | 47000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81H473MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 50[V] | 47000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E473KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 47000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E473MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 47000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H473KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 47000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H473MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 47000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR72A473KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 47000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR72A473MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 47000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81H563KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 50[V] | 56000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E563KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 56000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H563KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 56000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR72A563KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 56000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81H683KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 50[V] | 68000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81H683MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 50[V] | 68000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E683KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 68000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E683MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 68000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H683KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 68000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H683MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 68000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR72A683KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 68000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR72A683MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 68000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81H823KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 50[V] | 82000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E823KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 82000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H823KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 82000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR72A823KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 82000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81H104KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 50[V] | 100000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR72A104KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 100[V] | 100000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E124KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 120000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL8YA124KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 35[V] | 120000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H124KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 120000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E154KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 150000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E154MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 150000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL8YA154KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 35[V] | 150000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL8YA154MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 35[V] | 150000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H154KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 150000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H154MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 150000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E184KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 180000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E184MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 180000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL8YA184KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 35[V] | 180000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL8YA184MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 35[V] | 180000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H184KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 180000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H184MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 180000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E224KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 220000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E224MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 220000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL8YA224KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 35[V] | 220000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL8YA224MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 35[V] | 220000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H224KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 220000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H224MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 220000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E274KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 270000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71C274KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 16[V] | 270000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E274KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 270000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E334KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 330000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E334MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 330000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL8YA334KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 35[V] | 330000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL8YA334MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 35[V] | 330000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71C334KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 16[V] | 330000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71C334MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 16[V] | 330000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R71E334KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 330000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E334KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 330000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E334MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 330000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R71H334KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 330000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H334KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 330000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R71H334MA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 330000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H334MA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 330000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E394KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 390000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71C394KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 16[V] | 390000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E394KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 390000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E474KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 470000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL8EH474KA07 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 50[V]_derating | 470000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL8YA474KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 35[V] | 470000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R71E474KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 470000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ219R71E474MA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 470000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81C564KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 16[V] | 560000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71C564KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 16[V] | 560000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E564KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 560000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81C684KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 16[V] | 680000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81C684MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 16[V] | 680000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E684KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 680000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E684MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 680000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71C684KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 16[V] | 680000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71C684MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 16[V] | 680000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E684KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 680000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E684MA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 680000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81C824KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 16[V] | 820000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BL81E824KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X8L(-55to150[deg]) | 25[V] | 820000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E824KA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 820000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BC72A105KE02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7S(-55to125[deg]) | 100[V] | 1000000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BC72A105ME02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7S(-55to125[deg]) | 100[V] | 1000000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71C105MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 16[V] | 1000000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E105MA12 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 1000000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71H105KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 1000000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E155KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 1500000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BD71H225KE02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7T(-55to125[deg]) | 50[V] | 2200000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BD7YA225KE02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7T(-55to125[deg]) | 35[V] | 2200000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71A225KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 10[V] | 2200000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71A225MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 10[V] | 2200000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71C225KA13 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 16[V] | 2200000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71C225MA13 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 16[V] | 2200000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E225KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 2200000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71E225MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 25[V] | 2200000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BD71H475KE02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7T(-55to125[deg]) | 50[V] | 4700000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71C475KA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 16[V] | 4700000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71C475MA01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 16[V] | 4700000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BC71C106KE02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7S(-55to125[deg]) | 16[V] | 10000000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BC71E106KE02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7S(-55to125[deg]) | 25[V] | 10000000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71A106KE01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 10[V] | 10000000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BR71A106ME01 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 10[V] | 10000000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]
GCJ21BD70J226ME02 | Resin external electrode for Powertrain/safety for Automotive [AEC-Q200] | 2012[mm]/0805[inch] | X7T(-55to125[deg]) | 6.3[V] | 22000000[pF] | +/-20[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]