--------------------------------------------------------------------------------
Library :MurataDynamicModel_C
Conponent name : GJ821_D
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of GJ821_D

PartNumber | tmpr | Type | Size | TempCharacteristics | RatedVoltage | Value | Tolerance | Dimensions | FreqRange
GJ821BR71H105KA12 | 25 | Acoustic noise reduction type | 2012[mm]/0805[inch] | X7R(-55to125[deg]) | 50[V] | 1000000[pF] | +/-10[%] | 2.0x1.25[mm] | 100[Hz]-6[GHz]