--------------------------------------------------------------------------------
Library :MurataDynamicModel_C
Conponent name : LLL03_D
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of LLL03_D

PartNumber | tmpr | Type | Size | TempCharacteristics | RatedVoltage | Value | Tolerance | Dimensions | FreqRange
LLL03TR61E333KE01 | 25 | LW reversed low ESL type | 0306[mm]/0102[inch] | X5R(-55to85[deg]) | 25[V] | 33000[pF] | +/-10[%] | 0.3x0.6[mm] | 100[Hz]-6[GHz]