create_constant_form("NULL","NULL",16,"NULL","NULL");
create_constant_form("LQW32FT130M2H","1:LQW32FT130M2H, Wound, 13000[nH], +/-20[%], 550[mA], 0.1[MHz]-20[GHz]:1",68,"1","LQW32FT130M2H");
create_constant_form("LQW32FT220M2H","2:LQW32FT220M2H, Wound, 22000[nH], +/-20[%], 430[mA], 0.1[MHz]-20[GHz]:2",68,"2","LQW32FT220M2H");

create_form_set("LQW32FT_2H_list" 
,"LQW32FT130M2H"
,"LQW32FT220M2H"
);

create_compound_form("LQW32FT_2H_compound","Discrete Optimize setting","DistLibForm",68,"%p opt{ discrete %1p to %2p by 1 }","%s, %1s to %2s",
create_parm("NOM","Nominal",32,"LQW32FT_2H_list",-1,prm("LQW32FT130M2H")),
create_parm("MIN","Minimum",32,"LQW32FT_2H_list",-1,prm("LQW32FT130M2H")),
create_parm("MAX","Maximum",32,"LQW32FT_2H_list",-1,prm("LQW32FT220M2H")));

create_form_set("LQW32FT_2H_list_opt","NULL" 
,"LQW32FT130M2H"
,"LQW32FT220M2H"
,"LQW32FT_2H_compound"
);



