--------------------------------------------------------------------------------
Library :muRataLibWeb_C
Conponent name : LLC15
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of LLC15

PartNumber | Type | Size | TempCharacteristics | RatedVoltage | Value | Tolerance | Dimensions | FreqRange
LLC15SD70E105ME01 | Low ESL for Powertrain/Safety for Automotive[AEC-Q200] | 1005[mm] | X7T(-55to125[deg]) | 2.5[V] | 1000000[pF] | +/-20[%] | 0.5x1.0[mm] | 100[Hz]-6[GHz]
LLC152D70G105ME01 | Low ESL for Powertrain/Safety for Automotive[AEC-Q200] | 1005[mm] | X7T(-55to125[deg]) | 4[V] | 1000000[pF] | +/-20[%] | 0.5x1.0[mm] | 100[Hz]-6[GHz]
LLC152D70E225ME01 | Low ESL for Powertrain/Safety for Automotive[AEC-Q200] | 1005[mm] | X7T(-55to125[deg]) | 2.5[V] | 2200000[pF] | +/-20[%] | 0.5x1.0[mm] | 100[Hz]-6[GHz]