--------------------------------------------------------------------------------
Library :muRataLibWeb_C
Conponent name : GJ832
-------------------------------------------------------------------------------- Jump to Murata website for the latest ADS library
Jump to Murata website for the product information of GJ832

PartNumber | Type | Size | TempCharacteristics | RatedVoltage | Value | Tolerance | Dimensions | FreqRange
GJ832ER7YA106KA12 | Acoustic noise reduction | 3225[mm]/1210[inch] | X7R(-55to125[deg]) | 35[V] | 10000000[pF] | +/-10[%] | 3.2x2.5[mm] | 100[Hz]-6[GHz]